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	DDR3L for every need: U-DIMM/VLP, U-DIMM/R-DIMM/VLP, R-DIMM/SO-DIMM 

	Premier Series DDR3L memory modules offer multiple form factors for various installation needs. All run at a reduced 1.35V compared to 1.5V on standard DDR3, with speeds up to 1600MHz. Whether in standard U-DIMM, very low profile modules (VLP), or small outline modules (SO-DIMM) for notebooks, all implement cutting edge technology that enables remarkable memory quality, stability, and reliability. All modules are produced in accordance with JEDEC and RoHS design and production standards, guaranteeing compatibility with every major computing platform. Each is also made with environmental protection and preservation in mind, and includes a lifetime ADATA warranty. 



	Features
	U-DIMM


VLP U-DIMM


R-DIMM


VLP R-DIMM


SO-DIMM




	· High speed up to 1600MHz
· Transfer bandwidths up to 12.8GB/s
· Energy efficient: save up to 10% compared to DDR3
· 6-layer PCB provides improved signal transfer and system stability
	


Specifications
	Type　
	U-DIMM
	VLP U-DIMM
	R-DIMM
	VLP R-DIMM 
	SO-DIMM 

	Form factor
	Standard
(1.18" height)
	Standard
(0.7" height)
	Standard
(1.18" height)
	Very low profile (0.7" height)
	Standard
(1.18" height)

	Suitable for
	Desktop
	Desktop / Thin client
	Enterprise servers / data centers
	Blade servers
	Notebook

	[bookmark: _GoBack]Interface
	240-pin
	240-pin
	240-pin
	240-pin
	204-pin

	Capacity
	2GB/4GB/8GB
	4GB/8GB
	4GB/8GB/16GB
	4GB/8GB
	2GB/8GB

	Rank
	Single / Dual
	Single / Dual
	Single / Dual
	Single / Dual
	Single / Dual

	Speed
	Up to 1600MHz

	VDD voltage
	1.35V

	CAS latency
	CL11

	Refresh
	Auto-refresh / self-refresh

	Operating temperature
	0°C-85°C

	RoHS
	Yes

	Standard
	JEDEC

	Warranty 
	Limited lifetime warranty


Ordering Information
	Product
	Capacity 
	Rank
	Voltage
	Data rate
	Speed
	CL
	Part number 

	U-DIMM
	2GB
	Single
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDU160022G11

	
	4GB
	Single
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDU1600W4G11

	
	8GB
	Dual
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDU1600W8G11

	VLP U-DIMM
	4GB
	Single
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDX1600W4G11

	
	8GB
	Dual
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDX1600W8G11

	R-DIMM
	4GB
	Single
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDR1600W4G11

	
	8GB
	Dual
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDR1600W8G11

	
	16GB
	Dual
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDR1600Y16G11

	VLP R-DIMM
	4GB
	Single
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDV1600W4G11

	
	8GB
	Dual
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDV1600W8G11

	  SO-DIMM
	2GB
	Single
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDS160022G11

	
	8GB
	Dual
	1.35V
	1600MT/s
	PC3L-12800
	CL = 11
	ADDS1600W8G11



[image: ]
image2.png





image3.png





image4.png





image5.png
Yapara s CE X

ADDV1800V18G11-888D |||
DDRSL 1600(11) 16GX18 VLP-R |\,
10341041

0200134431






image6.png





image1.png
Fantastic Performance
Value Solutions

Premier Series 8 Gigabyte DDR3L-1600 240Pin
Unbuffered-DIMM Memory





image7.jpeg
’iADATN




image8.jpg




